** **

**FIAT 500 TECHNICAL SPECIFICATIONS**

**2012 MODEL YEAR**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **FIAT 500** | **1.2 69hp** | **0.9 TwinAir 85hp** | | **1.4 TJet Abarth** |
| Engine | 4-cyl 16v 1,242cc | 2-cyl 8v Turbo 875cc | | 4-cyl 16v Turbo 1,348cc |
| Power (hp) | 69 @ 5,500rpm | 85 @ 5,500rpm | | 135 @ 5,500rpm |
| Torque (Nm) | 102 @ 3,000rpm | 145 @ 1,900rpm | | 206 @ 3,000rpm |
| Transmission | 5-speed manual | 5-sp man | 5-sp MTA | 5-speed manual |
| 0-100 km/h | 12.9 seconds | 11.0 secs | 11.0 secs | 7.9 seconds |
| Max. Speed | 159km/h | 174 m/h | 174km/h | 205km/h |
| CO2 emissions | 115g/km | 95g/km | 92g/km | 155g/km |
| Economy Urban | 5.7L/100km | 4.9L/100km | 4.6L/100km | 8.5L/100km |
| Economy Motorway | 4.3L/100km | 3.7L/100km | 3.6L/100km | 5.4L/100km |
| Economy Combined | 4.8L/100km | 4.1L/100km | 4.0L/100km | 6.5L/100km |
| Kerb Weights | 865kg | 930kg | 940kg | 1,035kg |
| Brakes Front (mm) | 257 X 12 (solid discs) | 240 X 22 (vented discs) | | 284 X 22 (vented discs) |
| Brake Discs (mm) | 180 (drums) | 203 (drums) | | 240 X 11 (disc) |
| Dimensions (mm) | L 3,546 x H 1,488 x W 1627 x Wheelbase 2,300 | | | 3,657 1,480 1,627 2,300 |
| Suspension (front) | MacPherson struts with coil springs, dual-phase shock absorbers, anti-roll bar | | | |
| Suspension (rear) | Torsion beam with coil springs | | | |
| Capacities | 4 Seats / 35-litre Fuel Tank / Cargo Volume 185 – 550 litres | | | |
| Warranty/Service | 5 Years or 100,000km /Annual or 30,000km | | | |
| Safety | 5-Star EuroNCAP / 7 airbags / 2 rear ISOFIX / Switchable front passenger airbag | | | |