 

**2012 Chrysler 300C**

|  |  |  |  |
| --- | --- | --- | --- |
| Engine | 3,604cc V6 VVT | 2,987cc V6 CRD | 2,987cc V6 CRD |
| Power | 286hp @ 6,350rpm | 190hp @ 4,000rpm | 236hp @ 4,000rpm |
| Torque | 340Nm @ 4,650rpm | 440Nm @ 1,600-2,800 | 550Nm @ 1,800-2,800 |
| Transmission | 8-speed auto, RWD | 5-speed auto, RWD | 5-speed auto, RWD |
| Top Speed | 240 km/h | 220 km/h | 230 km/h |
| 0-100km/h | 7.7 seconds | 9.7 seconds | 7.8 seconds |
| Economy(Urban) | 13.9L/100km | 9.5L/100km | 9.5L/100km |
| Economy(Motorway) | 6.7L/100km | 5.7L/100km | 5.7L/100km |
| Economy(Combined) | 9.4L/100km | 7.1L/100km | 7.1L/100km |
| CO2 Emissions | 219g/km VRT Band F | 185g/km VRT Band E | 185g/km VRT Band E |
| Suspension (Front) | Multilink, coil spring, gas-charged shock absorbers, anti-roll bar | | |
| Suspension (Rear) | Multilink, coil spring, gas-charged shock absorbers, anti-roll bar | | |
| Steering | Rack and Pinion, 11.5m turning circle | | |
| Brakes | Ventilated Discs (f) 345 x 28mm, (r) 320 x 22mm, Advanced ESP | | |
| Tyres | 235/55 R18 (SR) 245/45 ZR20 (Limited) | | |
| Dimensions | L 5,066mm x H 1,488mm x W 1,902mm Wheelbase 3,052mm | | |
| Weight | 1,801kg | 1,963kg | 1,963kg |
| Luggage Capacity | 462 litres | | |