 

**2012 Chrysler Grand Voyager**

|  |  |
| --- | --- |
| **Chrysler Grand Voyager Technical Specification** | |
| Engine | 2,777cc, 4-cyl, 16V, Turbo Diesel, Common Rail Direct Injection |
| Power/Torque | 163hp @ 3,800rpm / 360Nm @ 1,600 – 3,000rpm |
| Transmission | 6-speed automatic, front wheel drive |
| Performance | 0-100km/h in 12.8 seconds, 185km/h top speed |
| Economy | Urban 11.0L/100km, Motorway 7.0L/100km, Combined (8.4L/100km) |
| CO2 Emissions | 222gkm, VRT Band F, Road Tax €1,050 |
| Suspension (Front) | MacPherson strut, coil spring, gas-charged shock absorbers, anti-roll bar |
| Suspension (Rear) | Torsion-beam axle, coil springs, gas-charged shock absorbers, trackbar |
| Steering | Rack and Pinion, 3.14 turns lock-to-lock, 11.91m turning circle |
| Brakes | Ventilated Discs front, Solid Discs Rear, ABS, EBD, ETC and ESP |
| Tyres | 225/65R16 (Touring) 225/65R17 (Limited) |
| Dimensions | L 5,143mm x H 1,750mm x W 1,954mm Wheelbase 3,078mm |
| Weight | 2,305kg (Max Towing Weight 1,600kg, Max Roof Rail Load 68kg) |
| Luggage Capacity | 756 litres - 3,296 litres (2,054 litres in four-seat mode) |